\subsection{Compute a curve interpolating a straight line between two points.}
\funclabel{s1602}
\begin{minipg1}
To make a straight line represented as a B-spline curve between two points.
\end{minipg1}\\ \\
SYNOPSIS\\
        \>void s1602(\begin{minipg3}
                {\fov startpt}, {\fov endpt}, {\fov order}, {\fov dim}, {\fov startpar}, {\fov endpar},
                {\fov curve}, {\fov stat})
                \end{minipg3}\\[0.3ex]
                \>\>    double  \>      {\fov startpt}[\,];\\
                \>\>    double  \>      {\fov endpt}[\,];\\
                \>\>    int     \>      {\fov order};\\
                \>\>    int     \>      {\fov dim};\\
                \>\>    double  \>      {\fov startpar};\\
                \>\>    double  \>      *{\fov endpar};\\
                \>\>    SISLCurve       \>      **{\fov curve};\\
                \>\>    int     \>      *{\fov stat};\\
\newpagetabs
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov startpt}  \> - \> Start point of the straight line\\
        \>\>    {\fov endpt}    \> - \> End point of the straight line\\
        \>\>    {\fov order}    \> - \> The order of the curve to be made.\\
        \>\>    {\fov dim}      \> - \> The dimension of the geometric space\\
        \>\>    {\fov startpar} \> - \> Start value of the parameterization of the curve\\
\\
        \>Output Arguments:\\
        \>\>    {\fov endpar }\> - \>   Parameter value used at the end of the curve\\
        \>\>    {\fov curve}    \> - \> Pointer to the B-spline curve\\
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $> 0$   : warning\\
                \>\>\>\>\>              $= 0$   : ok\\
                \>\>\>\>\>              $< 0$   : error\\
\\
EXAMPLE OF USE\\
                \>      \{ \\
                \>\>    double          \>{\fov startpt}[2];\\
                \>\>    double          \>{\fov endpt}[2];\\
                \>\>    int             \>{\fov order};\\
                \>\>    int             \>{\fov dim};\\
                \>\>    double          \>{\fov startpar};\\
                \>\>    double          \>{\fov endpar};\\
                \>\>    SISLCurve               \>*{\fov curve};\\
                \>\>    int             \>{\fov stat};\\
                \>\>    \ldots \\
        \>\>s1602(\begin{minipg4}
                {\fov startpt}, {\fov endpt}, {\fov order}, {\fov dim},
        {\fov startpar}, \&{\fov endpar}, \&{\fov curve}, \&{\fov stat});
                        \end{minipg4}\\
                \>\>    \ldots \\
                \>      \} \\
\end{tabbing}
