\subsection{Compute a fillet curve based on parameter value.}
\funclabel{s1607}
\begin{minipg1}
  To calculate a fillet curve between two curves. The start and end point
  for the fillet is given as one parameter value for each of the
  curves.
  The output is represented as a B-spline curve.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1607(\begin{minipg3}
        {\fov curve1}, {\fov curve2}, {\fov epsge}, {\fov end1}, {\fov fillpar1}, {\fov end2}, {\fov fillpar2},
        {\fov filltype}, {\fov dim}, {\fov order}, {\fov newcurve}, {\fov stat})
                \end{minipg3}\\[0.3ex]
                \>\>    SISLCurve       \>      *{\fov curve1};\\
                \>\>    SISLCurve       \>      *{\fov curve2};\\
                \>\>    double  \>      {\fov epsge};\\
                \>\>    double  \>      {\fov end1};\\
                \>\>    double  \>      {\fov fillpar1};\\
                \>\>    double  \>      {\fov end2};\\
                \>\>    double  \>      {\fov fillpar2};\\
                \>\>    int     \>      {\fov filltype};\\
                \>\>    int     \>      {\fov dim};\\
                \>\>    int     \>      {\fov order};\\
                \>\>    SISLCurve       \>      **{\fov newcurve};\\
                \>\>    int     \>      *{\fov stat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov curve1}   \> - \> The first input curve.\\
        \>\>    {\fov curve2}   \> - \> The second input curve.\\
        \>\>    {\fov epsge}    \> - \> Geometry resolution.\\
        \>\>    {\fov end1}     \> - \> \begin{minipg2}
                        Parameter value on the first curve. The parameter fillpar1 divides the first curve in two pieces. End1 is used to select which of these pieces the fillet should extend.
                                \end{minipg2}\\[0.8ex]
        \>\>    {\fov fillpar1}\> - \>  \begin{minipg2}
                        Parameter value of the start point of the fillet
                                on the first curve.
                                \end{minipg2}\\[0.8ex]
        \>\>    {\fov end2}     \> - \> \begin{minipg2}
                        Parameter value on the second curve indicating that
                        the part of the curve lying on this side of fillpar2
                                shall not be replaced by the fillet.
                                \end{minipg2}\\[0.3ex]
        \>\>    {\fov fillpar2}\> - \>  \begin{minipg2}
                        Parameter value of the start point of the fillet
                                on the second curve.
                                \end{minipg2}\\
\newpagetabs
        \>\>    {\fov filltype}\> - \>  Indicator of the type of fillet.\\
                \>\>\>\>\>      $=1$ : \>\begin{minipg5}
                                Circle approximation, interpolating tangent on first
                                curve, not on curve 2.
                                \end{minipg5}\\[0.3ex]
                \>\>\>\>\>      $=2$ : \>\begin{minipg5}
                                Conic approximation if possible,
                                \end{minipg5}\\
                \>\>\>\>\>      else : \>\begin{minipg5}
                                polynomial segment.
                                \end{minipg5}\\
        \>\>    {\fov dim}      \> - \> Dimension of space.\\
        \>\>    {\fov order}    \> - \> Order of the fillet curve, which is not always used.\\
\\
        \>Output Arguments:\\
        \>\>    {\fov newcurve}\> - \> Pointer to the B-spline fillet curve.\\
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $> 0$   : warning\\
                \>\>\>\>\>              $= 0$   : ok\\
                \>\>\>\>\>              $< 0$   : error\\
\\
EXAMPLE OF USE\\
                \>      \{ \\
                \>\>    SISLCurve       \>      *{\fov curve1};\\
                \>\>    SISLCurve       \>      *{\fov curve2};\\
                \>\>    double  \>      {\fov epsge};\\
                \>\>    double  \>      {\fov end1};\\
                \>\>    double  \>      {\fov fillpar1};\\
                \>\>    double  \>      {\fov end2};\\
                \>\>    double  \>      {\fov fillpar2};\\
                \>\>    int     \>      {\fov filltype};\\
                \>\>    int     \>      {\fov dim};\\
                \>\>    int     \>      {\fov order};\\
                \>\>    SISLCurve       \>      *{\fov newcurve};\\
                \>\>    int     \>      {\fov stat};\\
                \>\>    \ldots \\
        \>\>s1607(\begin{minipg4}
        {\fov curve1}, {\fov curve2}, {\fov epsge}, {\fov end1}, {\fov fillpar1}, {\fov end2}, {\fov fillpar2},
        {\fov filltype}, {\fov dim}, {\fov order}, \&{\fov newcurve}, \&{\fov stat});
                        \end{minipg4}\\
                \>\>    \ldots \\
                \>      \} \\
\end{tabbing}
