\subsection{Find the topology for the intersection between two surfaces.}
\funclabel{s1859}
\begin{minipg1}
  Find all intersections between two surfaces.
  Intersection curves are described by guide points.
  To produce the intersection curves use s1310() described on page \pageref{s1310}.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1859    (\begin{minipg3}
                {\fov surfl}, {\fov surf2}, {\fov epsco}, {\fov epsge}, {\fov numintpt},
                {\fov pointpar1}, {\fov pointpar2}, \linebreak {\fov numintcr}, {\fov intcurves},
                {\fov stat})
                \end{minipg3}\\[0.3ex]
                \>\>    SISLSurf        \>      *{\fov surf1};\\
                \>\>    SISLSurf        \>      *{\fov surf2};\\
                \>\>    double  \>      {\fov epsco};\\
                \>\>    double  \>      {\fov epsge};\\
                \>\>    int     \>      *{\fov numintpt};\\
                \>\>    double  \>      **{\fov pointpar1};\\
                \>\>    double  \>      **{\fov pointpar2};\\
                \>\>    int     \>      *{\fov numintcr};\\
                \>\>    SISLIntcurve\>  ***{\fov intcurves};\\
                \>\>    int     \>      *{\fov stat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov surf1}\> - \>     \begin{minipg2}
                                Pointer to the first surface.
                                \end{minipg2}\\
        \>\>    {\fov surf2}\> - \>     \begin{minipg2}
                                Pointer to the second surface.
                                \end{minipg2}\\
        \>\>    {\fov epsco}\> - \>     \begin{minipg2}
                                Computational resolution (not used).
                                \end{minipg2}\\
        \>\>    {\fov epsge}\> - \>     \begin{minipg2}
                                Geometry resolution.
                                \end{minipg2} \\
\\
        \>Output Arguments:\\
        \>\>    {\fov numintpt}\> - \>  \begin{minipg2}
                                Number of single intersection points.
                                \end{minipg2}\\
        \>\>    {\fov pointpar1}\> - \>\begin{minipg2}
                                Array containing the parameter values of the single
                                intersection points in the parameter plane of the
                                first surface. The points lie in sequence. Intersection
                                curves are stored in intcurves.
                                \end{minipg2}\\[0.8ex]
        \>\>    {\fov pointpar2}\> - \>\begin{minipg2}
                                Array containing the parameter values of the single
                                intersection points in the parameter plane of the
                                second surface.
                                \end{minipg2}\\[0.8ex]
        \>\>    {\fov numintcr}\> - \>  \begin{minipg2}
                                Number of intersection curves.
                                \end{minipg2}\\
        \>\>    {\fov intcurves}\> - \>\begin{minipg2}
                                Array containing description of the intersection
                                curves. The curves are only described
                                by start points and end points (guide
                                points) in
                                the parameter planes of the surfaces.
                                The curve pointers point to
                                nothing.
                                \end{minipg2}\\[0.3ex]
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $> 0$   : warning\\
                \>\>\>\>\>              $= 0$   : ok\\
                \>\>\>\>\>              $< 0$   : error\\
\newpagetabs
EXAMPLE OF USE\\
                \>      \{ \\
                \>\>    SISLSurf        \>      *{\fov surf1};\\
                \>\>    SISLSurf        \>      *{\fov surf2};\\
                \>\>    double  \>      {\fov epsco};\\
                \>\>    double  \>      {\fov epsge};\\
                \>\>    int     \>      {\fov numintpt};\\
                \>\>    double  \>      *{\fov pointpar1};\\
                \>\>    double  \>      *{\fov pointpar2};\\
                \>\>    int     \>      {\fov numintcr};\\
                \>\>    SISLIntcurve\>  **{\fov intcurves};\\
                \>\>    int     \>      {\fov stat};\\
                \>\>    \ldots \\
        \>\>s1859(\begin{minipg4}
                {\fov surfl}, {\fov surf2}, {\fov epsco}, {\fov epsge}, \&{\fov numintpt},
                \&{\fov pointpar1}, \&{\fov pointpar2}, \&{\fov numintcr}, \&{\fov intcurves},
                \&{\fov stat});
                \end{minipg4}\\
                \>\>    \ldots \\
                \>      \}
\end{tabbing}
