\section{Pick a Part of a Surface.}
\funclabel{s1001}
\begin{minipg1}
  To pick a part of a surface.
  The surface produced will always be k-regular, i.e.\ with
  k-tupple start/end knots.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1001(\begin{minipg3}
          {\fov ps},  {\fov min1},  {\fov min2},  {\fov max1},  {\fov max2},  {\fov rsnew},  {\fov jstat})
        \end{minipg3}\\[0.3ex]
        \>\>    SISLSurf \> *{\fov ps};\\
        \>\>    double   \> {\fov min1};\\
        \>\>    double   \> {\fov min2};\\
        \>\>    double   \> {\fov max1};\\
        \>\>    double   \> {\fov max2};\\
        \>\>    SISLSurf \> **{\fov rsnew};\\
        \>\>    int      \> *{\fov jstat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov ps}\> - \>  \begin{minipg2}
                     Surface to pick a part of.
                               \end{minipg2}\\
        \>\>    {\fov min1}\> - \>  \begin{minipg2}
                     Minimum value in first parameter direction.
                               \end{minipg2}\\
        \>\>    {\fov min2}\> - \>  \begin{minipg2}
                     Minimum value in second parameter direction.
                               \end{minipg2}\\
        \>\>    {\fov max1}\> - \>  \begin{minipg2}
                     Maximum value in first parameter direction.
                               \end{minipg2}\\
        \>\>    {\fov max2}\> - \>  \begin{minipg2}
                     Maximum value second parameter direction.
                               \end{minipg2}\\
\\
        \>Output Arguments:\\
        \>\>    {\fov rsnew}\> - \>  \begin{minipg2}
                     The new, picked surface.
                               \end{minipg2}\\
        \>\>    {\fov jstat} \> - \> Status messages\\
                \>\>\>\>\>           $> 0$ \> : Warning.\\
                \>\>\>\>\>           $= 0$ \> : Ok.\\
                \>\>\>\>\>           $< 0$ \> : Error.\\
\\
EXAMPLE OF USE\\
        \>      \{ \\
        \>\>    SISLSurf \> *{\fov ps};\\
        \>\>    double   \> {\fov min1};\\
        \>\>    double   \> {\fov min2};\\
        \>\>    double   \> {\fov max1};\\
        \>\>    double   \> {\fov max2};\\
        \>\>    SISLSurf \> *{\fov rsnew} = NULL;\\
        \>\>    int      \> {\fov jstat} = 0;\\
        \>\>    \ldots \\
        \>\>s1001(\begin{minipg4}
          {\fov ps},  {\fov min1},  {\fov min2},  {\fov max1},  {\fov max2}, \&{\fov rsnew},  \&{\fov jstat});
        \end{minipg4}\\
        \>\>    \ldots \\
        \>      \}
\end{tabbing}
