\subsection{Subdivide a curve at a given parameter value.}
\funclabel{s1710}
\begin{minipg1}
  Subdivide a curve at a given parameter value.\\
  NOTE: When the curve is periodic (i.e.\ when the {\fov cuopen} flag of
  the curve has value $=-1$), this function will return only ONE curve
  through {\fov rcnew1}. This curve is the same geometric curve as {\fov pc1},
  but is represented on a closed basis, i.e.\ with k-tuple start/end
  knots and coinciding start/end coefficients.
  The {\fov cuopen} flag of the curve will then be set to closed ($=0$)
  and a status value {\fov jstat} equal to 2 will be returned.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1710(\begin{minipg3}
          {\fov pc1},  {\fov apar},  {\fov rcnew1},  {\fov rcnew2},  {\fov jstat})
        \end{minipg3}\\[0.3ex]
        \>\>    SISLCurve \> *{\fov pc1};\\
        \>\>    double    \> {\fov apar};\\
        \>\>    SISLCurve \> **{\fov rcnew1};\\
        \>\>    SISLCurve \> **{\fov rcnew2};\\
        \>\>    int       \> *{\fov jstat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov pc1}  \> - \> The curve to subdivide.\\
        \>\>    {\fov apar} \> - \> Parameter value at which to subdivide.\\
\\
        \>Output Arguments:\\
        \>\>    {\fov rcnew1} \> - \> First part of the subdivided curve.\\
        \>\>    {\fov rcnew2} \> - \>
        \begin{minipg2}
          Second part of the subdivided curve.
          If the parameter value is at the end of a
          curve NULL pointers might be returned
        \end{minipg2}\\[0.8ex]
        \>\>    {\fov jstat} \> - \> Status messages\\
                      \>\>\>\>\> $= 5$      : \begin{minipg5}
                                                Parameter value at end of
                                                curve, $rcnew1$=NULL or
                                                {\fov rcnew2}=NULL.
                                              \end{minipg5}\\[0.8ex]
                      \>\>\>\>\> $= 2$      : {\fov pc1} periodic,
                                              {\fov rcnew2}=NULL.\\
                      \>\>\>\>\> $> 0$      : Warning.\\
                      \>\>\>\>\> $= 0$      : Ok.\\
                      \>\>\>\>\> $< 0$      : Error.\\
\newpagetabs
EXAMPLE OF USE\\
        \>      \{ \\
        \>\>    SISLCurve \> *{\fov pc1};\\
        \>\>    double    \> {\fov apar};\\
        \>\>    SISLCurve \> *{\fov rcnew1} = NULL;\\
        \>\>    SISLCurve \> *{\fov rcnew2} = NULL;\\
        \>\>    int       \> {\fov jstat} = 0;\\
        \>\>    \ldots \\
        \>s1710(\begin{minipg4}
          {\fov pc1},  {\fov apar}, \&{\fov rcnew1}, \&{\fov rcnew2}, \&{\fov jstat});
        \end{minipg4}\\
        \>\>    \ldots \\
        \>      \}
\end{tabbing}
