\subsection{Compute a surface using the input points as
control vertices, automatic parameterization.}
\funclabel{s1620}
\begin{minipg1}
  To calculate a surface using the input points as
  control vertices. The parametrization is calculated
  according to {\fov ipar}.
  The output is represented as a B-spline surface.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1620(\begin{minipg3}
          {\fov epoint}, {\fov inbpnt1}, {\fov inbpnt2}, {\fov ipar},
          {\fov iopen1}, {\fov iopen2}, {\fov ik1}, {\fov ik2}, {\fov idim}, {\fov rs}, {\fov jstat})
        \end{minipg3}\\[0.3ex]
        \>\>    double \> {\fov epoint}[\,];\\
        \>\>    int    \> {\fov inbpnt1};\\
        \>\>    int    \> {\fov inbpnt2};\\
        \>\>    int    \> {\fov ipar};\\
        \>\>    int    \> {\fov iopen1};\\
        \>\>    int    \> {\fov iopen2};\\
        \>\>    int    \> {\fov ik1};\\
        \>\>    int    \> {\fov ik2};\\
        \>\>    int    \> {\fov idim};\\
        \>\>    SISLSurf \> **{\fov rs};\\
        \>\>    int    \> *{\fov jstat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov epoint} \> - \>
        \begin{minipg2}
          The array containing the points to be used as
          controlling vertices of the B-spline surface.
        \end{minipg2}\\
        \>\>    {\fov inbpnt1} \> - \> The number of points in first
                                       parameter direction.\\
        \>\>    {\fov inbpnt2} \> - \> The number of points in second
                                       parameter direction.\\
        \>\>    {\fov ipar} \> - \> Flag showing the desired
                                    parametrization to be used:\\
                 \>\>\>\> $= 1$ \>:
                 \begin{minipg5}
                   Mean accumulated cord-length
                   parameterization.
                 \end{minipg5}\\[0.8ex]
                 \>\>\>\> $= 2$ \>: Uniform parametrization.\\
        \>\>    {\fov iopen1} \> - \>
          Open/close condition in the first parameter direction:\\
          \>\>\>\> $=1$ \>: Open.\\
          \>\>\>\> $=0$ \>: Closed. \\
          \>\>\>\> $=-1$ \>: Closed and periodic.\\
\newpagetabs
        \>\>    {\fov iopen2} \> - \>
          Open/close condition in the second parameter direction:\\
          \>\>\>\> $=1$ \>: Open.\\
          \>\>\>\> $=0$ \>: Closed. \\
          \>\>\>\> $=-1$ \>: Closed and periodic.\\
        \>\>    {\fov ik1} \> - \> The order of the surface in first direction.\\
        \>\>    {\fov ik2} \> - \> The order of the surface in second direction.\\
        \>\>    {\fov idim} \> - \> The dimension of the space.\\
\\
        \>Output Arguments:\\
        \>\>    {\fov rs} \> - \> Pointer to the B-spline surface.\\
         \>\>    {\fov jstat} \> - \> Status message\\
                \>\>\>\> $< 0$ \>: Error.\\
                \>\>\>\> $= 0$ \>: Ok.\\
                \>\>\>\> $> 0$ \>: Warning.\\
\\
EXAMPLE OF USE\\
        \>      \{ \\
        \>\>    double \> {\fov epoint}[300];\\
        \>\>    int    \> {\fov inbpnt1} = 10;\\
        \>\>    int    \> {\fov inbpnt2} = 10;\\
        \>\>    int    \> {\fov ipar};\\
        \>\>    int    \> {\fov iopen1};\\
        \>\>    int    \> {\fov iopen2};\\
        \>\>    int    \> {\fov ik1};\\
        \>\>    int    \> {\fov ik2};\\
        \>\>    int    \> {\fov idim} = 3;\\
        \>\>    SISLSurf \> *{\fov rs} = NULL;\\
        \>\>    int    \> {\fov jstat} = 0;\\
        \>\>    \ldots \\
        \>\>s1620(\begin{minipg4}
          {\fov epoint}, {\fov inbpnt1}, {\fov inbpnt2}, {\fov ipar},
          {\fov iopen1}, {\fov iopen2}, {\fov ik1}, {\fov ik2}, {\fov idim}, \&{\fov rs}, \&{\fov jstat});
        \end{minipg4}\\
        \>\>    \ldots \\
        \>      \}
\end{tabbing}
