\subsection{Find a point on a 2D curve along a given direction.}
\funclabel{s1013}
\begin{minipg1}
  Find a point on a 2D curve along a given direction.
\end{minipg1}\\ \\
SYNOPSIS\\
        \>void s1013(\begin{minipg3}
        {\fov pcurve}, {\fov ang}, {\fov ang\_tol}, {\fov guess\_par}, {\fov iter\_par}, {\fov jstat})
      \end{minipg3}\\[0.3ex]
      \>\>      SISLCurve \>  *{\fov pcurve};\\
      \>\>      double    \>   {\fov ang};\\
      \>\>      double    \>   {\fov ang\_tol};\\
      \>\>      double    \>   {\fov guess\_par};\\
      \>\>      double    \>  *{\fov iter\_par};\\
      \>\>      int       \>  *{\fov jstat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov pcurve}    \> - \> Pointer to the curve.\\
        \>\>    {\fov ang}       \> - \> \begin{minipg2}
                                           The angle (in radians)
                                           describing the wanted
                                           \mbox{direction}.
                                         \end{minipg2}\\[0.8ex]
        \>\>    {\fov ang\_tol}  \> - \> The angular tolerance (in radians).\\
        \>\>    {\fov guess\_par}\> - \> Start parameter value on the curve.\\
\\
        \>Output Arguments:\\
        \>\>    {\fov iter\_par} \> - \> The parameter value found on the curve.\\
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $= 2$   : A minimum distance found.\\
                \>\>\>\>\>              $= 1$   : Intersection found.\\
                \>\>\>\>\>              $< 0$   : Error.\\
\\
EXAMPLE OF USE\\
        \>      \{ \\
        \>\>    SISLCurve \>  *{\fov pcurve};\\
        \>\>    double    \>  {\fov ang};\\
        \>\>    double    \>  {\fov ang\_tol};\\
        \>\>    double    \>  {\fov guess\_par};\\
        \>\>    double    \>  {\fov iter\_par};\\
        \>\>    int       \>  {\fov jstat};\\
        \>\>    \ldots \\
        \>\>s1013(\begin{minipg4}
        {\fov pcurve}, {\fov ang}, {\fov ang\_tol}, {\fov guess\_par}, \&{\fov iter\_par}, \&{\fov jstat});
      \end{minipg4}\\
      \>\>    \ldots \\
      \>      \}
\end{tabbing}
