\subsection{Calculate the weight point and rotational momentum of
               an area between a 2D curve and a 2D point.}
\funclabel{s1243}
\begin{minipg1}
To calculate the weight point and rotational momentum of
               an area between a 2D curve and a 2D point. The area is
               also calculated.
               When the curve is rotating counter-clockwise around the
               point, the area contribution is positive.
               When the curve is rotating clockwise around the point,
               the area contribution is negative.
               OBSERVE: FOR CALCULATION OF AREA ONLY, USE s1241().
\end{minipg1} \\ \\
SYNOPSIS\\
        \> void s1243(\begin{minipg3}
            {\fov pcurve},  {\fov point},  {\fov dim},  {\fov epsge},  {\fov weight},  {\fov area},  {\fov moment},  {\fov stat})
                \end{minipg3}\\
                \>\>    SISLCurve    \>  *{\fov pcurve};\\
                \>\>    double    \>  {\fov point}[\,];\\
                \>\>    int    \>  {\fov dim};\\
                \>\>    double    \>  {\fov epsge};\\
                \>\>    double    \>  {\fov weight}[\,];\\
                \>\>    double    \>  *{\fov area};\\
                \>\>    double    \>  *{\fov moment};\\
                \>\>    int    \>  *{\fov stat};\\
\\
ARGUMENTS\\
	\>Input Arguments:\\
        \>\>    {\fov pcurve}\> - \>  \begin{minipg2}
                     The 2D curve.
                               \end{minipg2}\\
        \>\>    {\fov point}\> - \>  \begin{minipg2}
                     The reference point.
                               \end{minipg2}\\
        \>\>    {\fov dim}\> - \>  \begin{minipg2}
                     Dimension of geometry (must be 2).
                               \end{minipg2}\\
        \>\>    {\fov epsge}\> - \>  \begin{minipg2}
                     Absolute geometrical tolerance.
                               \end{minipg2}\\
\\
	\>Output Arguments:\\
        \>\>    {\fov weight}\> - \>  \begin{minipg2}
                     Weight point.
                               \end{minipg2}\\
        \>\>    {\fov area}\> - \>  \begin{minipg2}
                     Area.
                               \end{minipg2}\\
        \>\>    {\fov moment}\> - \>  \begin{minipg2}
                     Rotational momentum.
                               \end{minipg2}\\
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $> 0$   : warning\\
                \>\>\>\>\>              $= 0$   : ok\\
                \>\>\>\>\>              $< 0$   : error\\
\\
EXAMPLE OF USE\\
		\>      \{ \\

                \>\>    SISLCurve    \>  *{\fov pcurve};\\
                \>\>    double    \>  {\fov point}[\,];\\
                \>\>    int    \>  {\fov dim};\\
                \>\>    double    \>  {\fov epsge};\\
                \>\>    double    \>  {\fov weight}[\,];\\
                \>\>    double    \>  *{\fov area};\\
                \>\>    double    \>  *{\fov moment};\\
                \>\>    int    \>  *{\fov stat};\\                \>\>    \ldots \\
        \>\>s1243(\begin{minipg4}
            {\fov pcurve},  {\fov point},  {\fov dim},  {\fov epsge},  {\fov weight},  {\fov area},  {\fov moment},  {\fov stat});
                \end{minipg4}\\
                \>\>    \ldots \\
		\>      \}
\end{tabbing}
