\subsection{Find the direction cone of a surface.}
\funclabel{s1987}
\begin{minipg1}
  Find the direction cone of a surface.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1987(\begin{minipg3}
          {\fov ps}, {\fov aepsge}, {\fov jgtpi}, {\fov gaxis}, {\fov cang}, {\fov jstat})
        \end{minipg3}\\[0.ex]
        \>\>    SISLSurf \> *{\fov ps};\\
        \>\>    double   \> {\fov aepsge};\\
        \>\>    int      \> *{\fov jgtpi};\\
        \>\>    double   \> **{\fov gaxis};\\
        \>\>    double   \> *{\fov cang};\\
        \>\>    int      \> *{\fov jstat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov ps}\> - \>  \begin{minipg2}
                     Surface to treat.
                               \end{minipg2}\\
        \>\>    {\fov aepsge}\> - \>  \begin{minipg2}
                     Geometry tolerance.
                               \end{minipg2}\\
\\
        \>Output Arguments:\\
        \>\>    {\fov jgtpi}\> - \>
        \begin{minipg2}
          To mark if the angle of the direction cone is
          greater than $\pi$.
        \end{minipg2}\\[0.8ex]
                \>\>\>\> $=0$ \> :
                \begin{minipg5}
                  The direction cone of the surface
                  is not greater than $\pi$ in any parameter direction.
                \end{minipg5}\\[0.8ex]
                \>\>\>\> $=1$ \> :
                \begin{minipg5}
                  The direction cone of the surface
                  is greater than $\pi$ in the first parameter direction.
                \end{minipg5}\\[0.8ex]
                \>\>\>\> $=2$ \> :
                \begin{minipg5}
                  The direction cone of the surface is greater
                  than $\pi$ in the second parameter direction.
                \end{minipg5}\\[0.8ex]
                \>\>\>\> $=10$ \> :
                \begin{minipg5}
                  The direction cone of a boundary curve of
                  the surface is greater than $\pi$ in the first
                  parameter direction.
                \end{minipg5}\\[0.8ex]
                \>\>\>\> $=20$ \> :
                \begin{minipg5}
                  The direction cone of a boundary curve of
                  the surface is greater than $\pi$ in the second
                  parameter direction.
                \end{minipg5}\\[0.8ex]
        \>\>    {\fov gaxis}\> - \>
        \begin{minipg2}
          Allocated array containing the coordinates of the
          centre of the cone. It is only computed if $jgtpi=0$.
        \end{minipg2}\\[0.8ex]
        \>\>    {\fov cang}\> - \>
        \begin{minipg2}
          The angle from the centre to the boundary of the
          cone. It is only computed if $jgtpi=0$.
        \end{minipg2}\\[0.8ex]
        \>\>    {\fov jstat}     \> - \> Status messages\\
                \>\>\>\>              $> 0$ \> : Warning.\\
                \>\>\>\>              $= 0$ \> : Ok.\\
                \>\>\>\>              $< 0$ \> : Error.\\
\newpagetabs
EXAMPLE OF USE\\
        \>      \{ \\
        \>\>    SISLSurf \> *{\fov ps};\\
        \>\>    double   \> {\fov aepsge};\\
        \>\>    int      \> {\fov jgtpi} = 0;\\
        \>\>    double   \> *{\fov gaxis} = NULL;\\
        \>\>    double   \> {\fov cang} = 0.0;\\
        \>\>    int      \> {\fov jstat} = 0;\\
        \>\>    \ldots \\
        \>\>s1987(\begin{minipg4}
          {\fov ps}, {\fov aepsge}, \&{\fov jgtpi}, \&{\fov gaxis}, \&{\fov cang}, \&{\fov jstat});
        \end{minipg4}\\
        \>\>    \ldots \\
        \>      \}
\end{tabbing}
