\subsection{Split a curve into two new curves.}
\funclabel{s1714}
\begin{minipg1}
  Split a curve in two parts at two specified parameter values. The
  first curve starts at {\fov parval1}. If the curve is open, the last
  part of the curve is translated so that the end of the curve joins the
  start.
\end{minipg1} \\
SYNOPSIS\\
        \>void s1714(\begin{minipg3}
        {\fov curve}, {\fov parval1}, {\fov parval2}, {\fov newcurve1}, {\fov newcurve2}, {\fov stat})
                \end{minipg3}\\[0.3ex]
                \>\>    SISLCurve       \>      *{\fov curve};\\
                \>\>    double  \>      {\fov parval1};\\
                \>\>    double  \>      {\fov parval2};\\
                \>\>    SISLCurve       \>      **{\fov newcurve1};\\
                \>\>    SISLCurve       \>      **{\fov newcurve2};\\
                \>\>    int     \>      *{\fov stat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov curve}    \> - \> The curve to split.\\
        \>\>    {\fov parval1}  \> - \> \begin{minipg2}
                                Start parameter value of the first new curve.
                                \end{minipg2}\\
        \>\>    {\fov parval2}  \> - \> \begin{minipg2}
                                Start parameter value of the second new curve.
                                \end{minipg2}\\
\\
        \>Output Arguments:\\
        \>\>    {\fov newcurve1}\> - \>\begin{minipg2}
                                The first new curve.
                                \end{minipg2}\\
        \>\>    {\fov newcurve2}\> - \>\begin{minipg2}
                                The second new curve.
                                \end{minipg2}\\
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $> 0$   : warning\\
                \>\>\>\>\>              $= 0$   : ok\\
                \>\>\>\>\>              $< 0$   : error\\
EXAMPLE OF USE\\
                \>      \{ \\
                \>\>    SISLCurve       \>      *{\fov curve};\\
                \>\>    double  \>      {\fov parval1};\\
                \>\>    double  \>      {\fov parval2};\\
                \>\>    SISLCurve       \>      *{\fov newcurve1};\\
                \>\>    SISLCurve       \>      *{\fov newcurve2};\\
                \>\>    int     \>      stat;\\
                \>\>    \ldots \\
        \>\>s1714(\begin{minipg4}
                {\fov curve}, {\fov parval1}, {\fov parval2}, \&{\fov newcurve1}, \&{\fov newcurve2}, \&{\fov stat});
                        \end{minipg4}\\
                \>\>    \ldots \\
                \>      \}
\end{tabbing}
