\subsection{Approximate a curve with a sequence of straight lines.}
\funclabel{s1613}
\begin{minipg1}
  To calculate a set of points on a curve. The straight lines between the
  points will not deviate more than {\fov epsge} from the curve at any
  point.  The generated points will have the same spatial dimension as
  the input curve.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1613(\begin{minipg3}
        {\fov curve}, {\fov epsge}, {\fov points}, {\fov numpoints}, {\fov stat})
                \end{minipg3}\\[0.3ex]
                \>\>    SISLCurve       \>      *{\fov curve};\\
                \>\>    double  \>      {\fov epsge};\\
                \>\>    double  \>      **{\fov points};\\
                \>\>    int     \>      *{\fov numpoints};\\
                \>\>    int     \>      *{\fov stat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov curve}    \> - \> \begin{minipg2}
                                The input curve.
                                \end{minipg2}\\
        \>\>    {\fov epsge}\> - \>     \begin{minipg2}
                                Geometry resolution, maximum distance allowed
                                between the curve and the straight lines that are to be
                                calculated.
                                \end{minipg2}\\[0.8ex]
        \>Output Arguments:\\
        \>\>    {\fov points}   \> - \> \begin{minipg2}
                                Calculated points,\\
                                (a vector of
                                $numpoints\times curve${\tt ->}$idim$ elements).
                                \end{minipg2}\\[0.3ex]
        \>\>    {\fov numpoints}\> - \>\begin{minipg2}
                                Number of calculated points.
                                \end{minipg2}\\
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $> 0$   : warning\\
                \>\>\>\>\>              $= 0$   : ok\\
                \>\>\>\>\>              $< 0$   : error\\
EXAMPLE OF USE\\
                \>      \{ \\
                \>\>    SISLCurve       \>      *{\fov curve};\\
                \>\>    double  \>      {\fov epsge};\\
                \>\>    double  \>      *{\fov points};\\
                \>\>    int     \>      {\fov numpoints};\\
                \>\>    int     \>      {\fov stat};\\
                \>\>    \ldots \\
        \>\>s1613(\begin{minipg4}
                {\fov curve}, {\fov epsge}, \&{\fov points}, \&{\fov numpoints}, \&{\fov stat});
                        \end{minipg4}\\
                \>\>    \ldots \\
                \>      \}
\end{tabbing}
