\subsection{Convert a surface of order up to four to a mesh of Coons
patches.}
\funclabel{s1388}
\begin{minipg1}
  To convert a surface of order less than or equal to 4 in both
  directions to a mesh of Coons patches with uniform parameterization.
  The function assumes that the surface is $C^1$ continuous.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1388(\begin{minipg3}
                        {\fov surf}, {\fov coons}, {\fov numcoons1}, {\fov numcoons2}, {\fov dim}, {\fov stat})
                \end{minipg3}\\[0.3ex]

                \>\>    SISLSurf        \>      *{\fov surf};\\
                \>\>    double  \>      **{\fov coons};\\
                \>\>    int     \>      *{\fov numcoons1};\\
                \>\>    int     \>      *{\fov numcoons2};\\
                \>\>    int     \>      *{\fov dim}\\
                \>\>    int     \>      *{\fov stat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov surf}     \> - \> \begin{minipg2}
                                Pointer to the surface that is to be converted
                                \end{minipg2}\\[0.8ex]
        \>Output Arguments:\\
        \>\>    {\fov coons}    \> - \> \begin{minipg2}
                                Array containing the (sequence of) Coons patches.
                                The total number of patches is
                                $numcoons1\times numcoons2$. The patches
                                are stored in sequence with $dim\times
                                16$ values for each patch. For each
                                corner of the patch we store in
                                sequence, positions, derivative in first
                                direction, derivative in second
                                direction, and twists.
                                \end{minipg2}\\[0.3ex]
        \>\>    {\fov numcoons1}\> - \> \begin{minipg2}
                                Number of Coons patches in first
                                parameter direction.
                                \end{minipg2}\\[0.3ex]
        \>\>    {\fov numcoons2}\> - \> \begin{minipg2}
                                Number of Coons patches in second
                                parameter direction.
                                \end{minipg2}\\[0.3ex]
        \>\>    {\fov dim}      \> - \> \begin{minipg2}
                                The dimension of the geometric space.
                                \end{minipg2}\\
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>      $= 1$   :\>\begin{minipg5}
                                        Order too high, surface interpolated.
                                        \end{minipg5}\\
                \>\>\>\>\>      $= 0$   :\> Ok.\\
                \>\>\>\>\>      $< 0$   :\> Error.\\
\newpagetabs
EXAMPLE OF USE\\
                \>      \{ \\
                \>\>    SISLSurf        \>      *{\fov surf};\\
                \>\>    double  \>      *{\fov coons};\\
                \>\>    int     \>      {\fov numcoons1};\\
                \>\>    int     \>      {\fov numcoons2};\\
                \>\>    int     \>      {\fov dim}\\
                \>\>    int     \>      {\fov stat};\\
                \>\>    \ldots \\
        \>\>s1388(\begin{minipg4}
                {\fov surf}, \&{\fov coons}, \&{\fov numcoons1}, \&{\fov numcoons2}, \&{\fov dim}, \&{\fov stat});
                        \end{minipg4}\\
                \>\>    \ldots \\
                \>      \}
\end{tabbing}
