\section{Turn the Direction of the Surface Normal Vector.}
\funclabel{s1440}
\begin{minipg1}
  Interchange the two parameter directions used in the mathematical
  description of a surface and thereby change the direction of the
  normal vector of the surface.
\end{minipg1} \\ \\
SYNOPSIS\\
        \>void s1440(\begin{minipg3}
                                {\fov surf}, {\fov newsurf}, {\fov stat})
                \end{minipg3}\\[0.3ex]

                \>\>    SISLSurf        \>      *{\fov surf};\\
                \>\>    SISLSurf        \>      **{\fov newsurf};\\
                \>\>    int     \>      *{\fov stat};\\
\\
ARGUMENTS\\
        \>Input Arguments:\\
        \>\>    {\fov surf}\> - \>      \begin{minipg2}
                                Pointer to the original surface.
                                \end{minipg2}\\
        \>Output Arguments:\\
        \>\>    {\fov newsurf}\> - \>   \begin{minipg2}
                                Pointer to the surface where the parameter
                                directions are interchanged.
                                \end{minipg2}\\[0.3ex]
        \>\>    {\fov stat}     \> - \> Status messages\\
                \>\>\>\>\>              $> 0$   : warning\\
                \>\>\>\>\>              $= 0$   : ok\\
                \>\>\>\>\>              $< 0$   : error\\
\\
EXAMPLE OF USE\\
                \>      \{ \\
                \>\>    SISLSurf        \>      *{\fov surf};\\
                \>\>    SISLSurf        \>      *{\fov newsurf};\\
                \>\>    int     \>      {\fov stat};\\
                \>\>    \ldots \\
        \>\>s1440(\begin{minipg4}
                {\fov surf}, \&{\fov newsurf}, \&{\fov stat});
                        \end{minipg4}\\
                \>\>    \ldots \\
                \>      \}
\end{tabbing}
